SMT-3222 & SMT-4022 PROFESSIONAL LARGE LCD MONITOR
TECHNICAL SPECIFICATIONS							SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS 

PART 2 – PRODUCTS

2.01	GENERAL

A.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.

B.	All systems and components shall have been thoroughly tested and proven in actual use.

C.	All systems and components shall be provided with an explicit manufacturer warranty.

2.02	SMT-3222 and SMT-4022 PROFESSIONAL LARGE LCD MONITORS 

A.	The SMT-3222 monitor shall have a 32” wide screen with protecting glass. It shall offer 1,366 x 1768 resolution with 4,000:1 high contrast ratio, 450cd/m2 high brightness, and 8ms response time. 

B.	The SMT-4022 monitor shall have a 40” wide screen with protecting glass. It shall offer 1,920 x 1,060 resolution with 4000:1 high contrast ratio, 450cd/m2 high brightness, and 8ms response time. 

C.	Both monitors shall offer 178 horizontal and vertical viewing angle; HDMI, DVI, RGB and composite inputs, anti-image retention mode and signal balance function for weak RGB signal.

D.	Both monitors shall offer built-in speaker; extended video wall format (1x5~5x5) and built-in fan to prevent overheating and image corruption.

E.	All operation and configuration menus shall be provided in several languages, including support English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese, Korean, Turkish, and Taiwanese.

2.03	GENERAL
A. Screen Size	
	1. SMT-3222	32”
	2. SMT-4022	40”
B. Max. Resolution	
	1. SMT-3222	1366 x 768
	2. SMT-4022	1920 x 1080
C. Pixel Pitch	
	1. SMT-3222	0.511x 0.511mm (Horizontal/Vertical)
	2. SMT-4022	0.46125 x 0.46125mm (H/V)
D. Brightness	450 cd/m2
E. Contrast Ratio	4,000:1 (Dynamic Contrast 40,000:1)
F. Response Time	8ms (G-to-G)
G. Viewing Angle	178°, 178° (H/V)
H. Panel Lamp Life	50,000 hours
I. Display Color	16.7 Million
J. Frequency 	30 ~ 81KHz (H), 56 ~ 85KHz (V)
K. Horizontal Resolution	600 TV lines
L. Comb Filter	3D
M. Sync Format	NTSC: 3.5, PAL:4.43, Secam

2.04	FEATURES
A. Screen Aspect Ratio	4:3 / 16:9
B. Languages	English, Spanish, French, German, Italian, Portuguese, Russian, Swedish, Chinese, Japanese, Korean, Turkish, Taiwanese
C. Front Panel Control	Menu, Adjust down/ up/ left/ right, Enter, Source, D. Menu, Power 
D. Speaker output	
	1. SMT-3222	10W (5W x 2 built in)
	2. SMT-4022	20W (10W x 2 built in)
E. Indicator	LED (power)
F. VESA Mounts 	
	1. SMT-3222	200 x 200 mm
	2. SMT-4022	400 x 600 mm

2.05	INPUT INTERFACE	
A. Video	1 Composite (RCA), 1 HDMI
B. PC	1 RGB (D-sub), 1 DVI, 1 RS-232
C. Audio	2 RCA

2.06	POWER
A. Requirement	AC 100-240v, 50/60 Hz
B. Consumption	
	1. SMT-3222	130 (typ), 143W (max)
	2. SMT-4022	180 (typ), 220W (max)

2.07	DIMENSIONS 
A. SMT-3222
	1. Without Stand	780 x 482 x 109 mm
	2. With Stand	780 x 545 x 311 mm
	3. Weight	13.7 KG
B. SMT-4022
	1. Without Stand	971 x 582 x 118.5 mm
	2. With Stand	971 x 643 x 311 mm
	3. Weight	19 KG

2.09	ACCESSORIES
A. Accessories	Remote Control, Battery x 2, Quick Setup Guide, Warranty Card, User’s Guide, Power Cord, RCA to BNC Cable
B. Optional Accessories	Foot Stand

2.10	CERTIFICATIONS
A. UL Listed
B. UL Listed to Canadian safety standards
C. CE mark
D. FCC mark

2.11	WARRANTY
A.	3 years, parts and labor.